IN-ROADWAY LIGHT ASSEMBLY

Effective Date: 08/20/2018

Document Identifier: CM-654-2.1-01

Printed copies are for reference only; they are not controlled. Latest version is on-line.

FDOT Traffic Engineering Research Laboratory (TERL) In-Roadway Light Assembly Compliance Matrix	By signing this form, the applicant declares that he/she has read and understands the provisions of Section 654 of the FDOT Standard Specifications for Road and Bridge Construction and all implemented modifications. The requirements listed on this matrix are derived from Section 654, and are the basis for determining a product’s compliance and its acceptability for use on Florida’s roads.

Date:	Click here to enter a date.	Applicant’s Name (print):
Manufacturer:
Item, Model No.:	Signature:

ID No	Section	Requirement	Item Comply? (Yes/No)	Comments (Applicant must provide information as indicated)	TERL Evaluation Method
1	654-2.1	In-roadway light assembly meets the physical and operational requirements of the latest edition of the Federal Highway Administration’s (FHWA) Manual on Uniform Traffic Control Devices (MUTCD), Chapter 4.	Provide a third party test report that demonstrates compliance with this requirement. The test report must meet the requirements of FDOT Product Certification Handbook (PCH), section 7.2.	Document Review
Indicate location of requested information in submittal.
2	In-roadway light assembly is normally dark until activated.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
3	In-roadway light assembly initiates operation only through pedestrian actuation via a pedestrian push-button.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
4	In-roadway light assembly ceases operation at a predetermined time after pedestrian actuation or, with passive detection, after the pedestrian clears the crosswalk.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
5	The duration of the predetermined active period is programmable and capable of matching the pedestrian clearance time for pedestrian signals as determined by MUTCD procedures.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Functional Inspection
Indicate location of requested information in submittal.
6	The timer controlling the flashing automatically resets each time a pedestrian call is received.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Functional Inspection
Indicate location of requested information in submittal.
7	In-roadway light assemblies must have a minimum luminance of 101 candelas and a minimum viewing angle of 20 degrees.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Functional Inspection
Indicate location of requested information in submittal.
8	654-2.4	Cabinet meets the applicable criteria of Specification 676 of the MSTCSD.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement. Alternately, provide the APL number if the cabinet is APL listed.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
9	Housing, unless a cabinet, is powder coat painted dull black (Federal Standard 595A-37038) with a reflectance value of 25 percent, or less, as measured by America Society for Testing and Material (ASTM) E1347.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
10	Cabinet and/or housing prevents unauthorized access.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
11	If pole-mount, assembly allows installation on a 4.5 inch outer diameter post.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
12	All assembly hardware including screws, nuts, bolts, and locking washers less than 5/8 inch in diameter, is constructed of passivated stainless steel Type 304 or Type 316 and meets the requirements of ASTM F593 and ASTM F594. All assembly hardware greater than or equal to 5/8 inch in diameter is galvanized.	Provide statement of conformance from hardware supplier that shows the product meets this requirement.	Document Review
Indicate location of requested information in submittal.
13	Carbon steel hardware meets the requirements of ASTM A307.	Provide statement of conformance from hardware supplier that shows the product meets this requirement.	Document Review
Indicate location of requested information in submittal.
14	Structural bolts meet the requirements of ASTM A325.	Provide statement of conformance from hardware supplier that shows the product meets this requirement.	Document Review
Indicate location of requested information in submittal.
15	654-2.5	Assembly operates on solar power or nominal voltage of 120 VAC. If assembly operates on voltage less than 120 VAC, an appropriate voltage converter is supplied.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Physical Inspection
Indicate location of requested information in submittal.
16	If the device is solar powered, it is designed to provide 10 days of continuous operation without sunlight; it automatically charges batteries and prevents overcharging or over-discharging; it includes a charge indicator and an AC/DC battery charger.	Provide product literature, specifications, user manual,or similar information that shows the product meets this requirement.	Document Review and Functional Inspection
Indicate location of requested information in submittal.
17	654-2.6	Electronic assembly operates as specified during and after being subjected to the transients, temperature, voltage, humidity, vibration, and shock tests described in National Electrical Manufacturers Association (NEMA) TS2, 2.2.7, 2.2.8, and 2.2.9.	Provide a third party test report that demonstrates compliance with this requirement. The test report must meet the requirements of FDOT PCH, section 7.2.	Document Review
Indicate location of requested information in submittal.
18	Electronics meet Federal Communications Commission (FCC), Title 47 Subpart B Section 15.	Provide a third party test report that demonstrates compliance with this requirement. The test report must meet the requirements of FDOT PCH, section 7.2.	Document Review
Indicate location of requested information in submittal.